ITEM 4 3 2 1

NUMBER DESCRIPTION MANUFACTURER MFG PART NUMBER QTY.

REVISIONS

1 710-03081-01 ASSY, ELECT-MECH, M20 ADAPTER, BUTTER STICK, AMBER N/A N/A 1

ECO REV. DESCRIPTION BY DATE

2 725-01312-01 ASSY, HARNESS, CABLE, LINEAR SENSORESTRIP N/A N/A 1

ECO-033387 01 INITIAL RELEASE EMT 12/19/2019

3 961-00021-01 LABEL, 5 SENSOR HEADSET, AMBER N/A N/A 1

D

D3 1 2 CCB BCENTER LABEL HORIZONTALLY & FROM APPROXIMATELY BOTTOM EDGE, 11mm AS SHOWN

TEXT ORIENTATION

**CONFIDENTIAL** THIS DOCUMENT AND THE DATA DISCLOSED HEREIN OR **DRAWN**

**DATE** WHEREWITH IS NOT TO BE REPRODUCED, USED, OR RD/EMT/DSF 1/3/2020 A11 DISCLOSED IN WHOLE OR IN PART TO ANYONE WITHOUT THE PERMISSION OF GOOGLE, INC.

**CHECKED**

**DATE** G. LEVINE 1/3/2020

43 SHEET 1 OF 1

100 Mayfield Avenue Mountain View CA 94043 UNLESS OTHERWISE SPECIFIED **ENGINEER** DIMENSIONS ARE IN MILLIMETERS

USA

A

TOLERANCES UNLESS OTHERWISE NOTED:

1.

FOR ASSEMBLY: REFER TO MPI-0306-00, ASSEMBLY INSTRUCTIONS. X X.X X.XX ANGLES

1.0 0.3 .1 .25

G. LEVINE 1/3/2020

THIRD ANGLE

**MATERIAL**

N/A

**TITLE**

ASSY, ELEC-MECH, M20 HEADSET, BUTTER STICK, AMBER

2.

PART REQUIRES PACKAGING TO PREVENT DAMAGE DURING SHIPMENT. PROJECTION

**FINISH**

1.6

N/A

**SIZE** BSURFACE ROUGHNESS

UNLESS OTHERWISE SPECIFIED

BREAK SHARP EDGES TO <0.4 MM

**DO NOT SCALE DRAWING**

1:10 710-03085-02 2 1

**PART NUMBER**

710-03085-02

**REV**

01

INTERPRET DRAWING PER ASME Y14.5-2009

**SCALE**

**FILE NAME**

**MASS (g):**

267.64